**Available pipe organ, built by Trent Buhr**



Left hand side of keyboard – Manual stops Right hand side of keyboard - Pedal stops:

All divided bass & treble except (Dulciana) Subbass 16'

Gedeckt 8’ Bourdon 8' (ext)

Dulciana 8’ Flute 4' (ext)

Prestant 4’

Principal 2’ Tremolo

Traverse Flute 4’

Quint/Tierce

Main casework is 64-1/2” wide by 32” deep plus 23” for pedalboard

Case is 85-1/2” tall plus 13” for molding at top (which is removable)

The bass windchests for the Pedal Subbass are each 6” x 24-1/2”.

Mechanical action for Manual, electromechanical action for Pedal stop